{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Setup","Data"],"not_rendered":{"macros":1},"read":"whole","date_system":"1900"}

{"sheet":"Setup","index":0,"n_rows":60,"n_cols":6,"rows_kept":60}
[]
[null,"Communications Port:","COM4",null,null,"e.g. Windows: COM4, Mac: /dev/cu.wchusbserialfd130"]
[null,"Baud Rate:",9600]
[null,"Approx Time Between Data Points:",1,"seconds"]
[]
[]
[]
[]
[null,"Windows: Press Control+Shift+Q to stop data acquisition."]
[null,"Mac: Edit any cell to stop data acquisition. Disable auto RESET on the Uno by wiring a 10 uF cap between RES and GND."]
[]
[null,"Make sure the serial text is in CSV format. For Mac, the baud rate should be 9600."]
{"$rows_empty":42}
[{"$nulls":3},-93.09]
[null,"\n3.30",3.3,5114924.5,-93.09]
[null,"\n3.30",5114924.5,-93.09]
[null,"\n3.30",5114924.5,-93.09]
[null,"\n3.30",5114924.5,-93.09]
[null,"\n3.30"]

{"sheet":"Data","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}